**8IM 1 Facial care machine**

**Use manual**

****

**First of all, let us express our gratitude to the customers who have purchased our instruments. This manual is written for customers to use this instrument better. I hope that the company's products and services will bring you respect and courtesy!**

**1:product description**

**Black Pearl——The most comprehensive introduction in history**

**1. Bubble head: vacuum negative pressure, with negative pressure to take away the dirt from the face, clean the face.**

**2. Shovel skin knife: clean, exfoliate, moisturize the skin.**

**3. Spray gun: high-pressure oxygen injection to replenish water, deep muscles into the skin layer, easier to absorb through the fine pores.**

**4. Wave head (face + eyes): Import the product to make the product more absorbed, fine pores, and smooth skin.**

**5. Eye head: improve the fine lines of the eyes, tighten and lift.**

**6. Hot and cold head: shrink pores, block nutrition, calm and repair.**

**7. Girl's line: Gua Sha, detoxification, lifting and firming contours, introduction of essence, shaping and diminishing fine lines**


**8. Radio frequency head: enhance firmness and promote the re-growth of collagen.**

****

****

****

****


****

**New technology slidabe LCD screen,Touch “ENter”**

**1:Cool and warm hammer head**

**The ice treatment allergy,enhance immunity,Skin tightening,shrinks pores,tightens skin,removes wrinkles**

**Promotes collagen hyperplasia,eliminates radness and sensitivity. Accelerate product absorption.**

****

****

**Operation steps for Cool and warm hammer head**

 Start



Stop

Click this for refrigeration

Click this for heating

This is the time to choose the ice hammer to work

**2：RF Lifting head**

****

**Operation steps for RF lifting head**

Start


Stop



This is to choose the strength of RF energy

This is the time to choose the radio frequency controller to work

**3：Eyes ultrasound head**

****

**4:Facial ultrasound head**

****


****

**5:Miro Bubble cleaner head**


****

****


**6:Miro Bubble cleaner head**

****

**7:Beauty head(lifting Head)**

****

**8:Water oxygen head**

****

**Precautions：**

**1: Before use, please fill the solution bottle with proper purified water or nutrient solution, and do not use tap water:**

**2: Pay attention to the liquid level of the waste bottle, please discard it in time to prevent damage to the instrument.**

**3: Use with caution if the skin stratum corneum is thin or the cheekbones are severely red.**

**4: People who have undergone facial surgery or deep exfoliation, but have not yet reached the recovery period, use it with caution.**

**5: After the operation, it is necessary to strengthen the hydration, and apply the hydrating mask continuously for a week. Do not use functional hydrating products.**

unsuitable people

**1. People with pacemakers or other similar electronic devices implanted in their bodies.**

**2. Pregnant women.**

**3. People who have taken oral isotretinoin therapy in the past 9 months (Accutane / Roaccutane / Oratane).**

**4. There are fillers inside. If gold wires are implanted on the face, it is not recommended.**

**5. Patients with severe heart disease, diabetes, and hyperthyroidism.**

**6. The surgical wound has not healed.**

**7. Patients with advanced tumors.**

**8. Women with intrauterine contraceptive devices.**

**9, do not do during menstrual period**

**Maintenance and repair**

**Managers must inspect the instruments and components.**

**1. Whether the power socket is reliably connected to the ground, if not, please replace the power socket.**

**2. Whether the power cord is deformed, broken, or disconnected: through visual inspection, whether the cord is deteriorated or deformed, if any, it may leak electricity and cause a fire. Please replace with a new power cord immediately.**

**3. Whether the control handle is abnormal or disconnected: Check whether the output is deteriorated or deformed by visual inspection. If there is any, please replace it when it is produced.**

**4. Please check whether the content of the prompt before using the instrument is correct. If it is not correct, please stop using it.**

**5. When cleaning the instrument, the dust must be wiped with a dry soft cloth, and the dirt must be wiped with a soft damp cloth. Before cleaning the instrument, you must turn off the power switch and disconnect the power cord.**

**6. When using for a long time (more than one year) to clean the dust inside the instrument, it should be done by professional maintenance personnel.**

**When the instrument is not in use, it should be placed in a ventilated and dry place, and the top of the instrument should be covered with a dust cover.**